Linear Screed Line

Product Specification Document

DATE: 16.07.2019 REF: PL-CW-PSDLSL01









# **Detailed Description**

The Linear Screed Line drain has been designed for concrete or screed floors and can be used on concrete slabs, planks and block and beam floors.

Versatility is its key feature, being available with one, two or three traps and a chance of horizontal and vertical outlets. The drain incorporates out TR50 trap which has a 50mm waterseal and is supported by a lifetime guarantee.

Available until a chance of stylish grill finishes, the Linear Screed Line will suit almost any application.

# **System Components**

Drain Body

Linear Grill

Brackets

# **Features and Benefits**

* Horizontal or vertical outlet
* Flow rate up to 68 L/min
* 50mm TR50 waterseal trap (manufactured to EN 274-1:2002)
* Height adjustable brackets and grill
* 360° rotatable outlet
* Variable trap positions (left, right and centre)
* Top access trap for easy maintenance
* Grill lengths available up to 2000mm
* Bespoke designs available on request
* Lifetime Guarantee.

**Product Guidance**

* Single, Double and Triple traps are available to cope with flow rates of up to 68 L/min
* All Linear Screed Line drains are manufactured with one trough size at 660mm and all lengths of grill are then fitted onto this trough
* The wall grill width is adjustable to allow for different wall thickness
* The height of the grill is adjustable in 1mm increments to suit tile thicknesses of between 6-20mm. Additional spacers are available on request for tiles thicker than 20mm
* Floor grill width: 58mm
* Wall grill width: 86mm
* All grills are manufactured from 1.4401 (316) grade stainless steel and are available in a solid, slotted, stone-infill or frameless finish
* All grill finishes are available in 15 standard lengths from 600mm–2000mm
* Bespoke grills can be manufactured for sizes that are in between or over standard sizes
* Fast track bespoke lengths manufactured and delivered in 3-4 days

# **Horizontal Trap**

* 50mm Waterseal
* 40mm ABS pipe connection
* The horizontal trap incorporates an adjustable ball joint, allowing for ease of installation
* The trap can be positioned centre, left or right handed
* It is accessible from the top for cleaning and maintenance
* Standard brackets allow drain adjustment from 138mm–218mm

# **Vertical Trap**

* 50mm Waterseal
* 50mm ABS pipe connection
* The vertical trap allows the outlet to be positioned through the slab and connected to a waste pipe below
* The trap can be positioned centre, left or right handed
* It is accessible from the top for cleaning and maintenance
* Standard brackets allow drain adjustment from 55-88mm
* Extra shallow brackets allow drain adjustment from 38-57mm

# **Options**

# **Waterproofing Membrane**

CCL Wetrooms Tilesure Waterproofing & Decoupling Membrane or Screedsure membrane is applied to the whole shower area plus an additional metre outside of the shower area. FWM (Flexible Wall Membrane) should applied to the walls of the shower area and overlapped onto the Tilesure/ Screedsure Reinforcing Tape specified separately).

# **Product Specification**

**Product reference Code Traps Flow Rate**

**Horizontal Trap**

Drain Body with Standard Brackets LSL-1H/ST 1 24 L/min

Drain Body with Standard Brackets LSL-2H/ST 2 41 L/min

Drain Body with Standard Brackets LSL-3H/ST 3 68 L/min

**Vertical Trap**

Drain Body with Standard Brackets LSL-1V/ST 1 24 L/min

Drain Body with Standard Brackets LSL-2V/ST 2 41 L/min

Drain Body with Standard Brackets LSL-3V/ST 3 68 L/min

Drain Body with Extra Shallow Brackets LSL-1V/ES 1 24 L/min

Drain Body with Extra Shallow Brackets LSL-2V/ES 2 41 L/min

Drain Body with Extra Shallow Brackets LSL-3V/ES 3 68 L/min

 **Grill Type**

**Product reference Code Length Grill Finish**

Linear Wall Grill SWG-600 600mm Add code for Grill Finish

 SWG-700 700mm

 SWG-800 800mm

 SWG-900 900mm

 SWG-1000 1000mm

 SWG-1100 1100mm

 SWG-1200 1200mm

 SWG-1300 1300mm

 SWG-1400 1400mm

 SWG-1500 1500mm

 SWG-1600 1600mm

 SWG-1700 1700mm

 SWG-1800 1800mm

 SWG-1900 1900mm

 SWG-2000 2000mm

 SWG-FT Bespoke

 SWG-BES Bespoke

Linear Floor Grill SFG-600 600mm Add code for Grill Finish

 SFG-700 700mm

 SFG-800 800mm

 SFG-900 900mm

 SFG-1000 1000mm

 SFG-1100 1100mm

 SFG-1200 1200mm

 SFG-1300 1300mm

 SFG-1400 1400mm

 SFG-1500 1500mm

**Grill Type**

**Product reference Code Length Grill Finish**

Linear Floor Grill SFG-1600 1600mm

 SFG-1700 1700mm

 SFG-1800 1800mm

 SFG-1900 1900mm

 SFG-2000 2000mm

 SFG-FT Bespoke

 SFG-BES Bespoke

.

Grill Finish Type A - Solid grill, grained

stainless steel with 5mm

gap around the grill.

Type B - Oblong slots, three

rows of oblong slots in a

grained stainless steel finish.

Type C - Square holes, three

rows of squares in a grained

stainless steel finish.

Type S8 – Stone-infill grill. Allows a

section of tile to be inserted to

provide a sleek continuous finish.

Suitable for 6-8mm stone/

porcelain tiles.

Type S12 – Stone-infill grill.

Suitable for 10.12mm stone/

porcelain tiles.

Type S20 – Stone-infill grill.

Suitable for 18-20mm stone/

porcelain tiles.

Type F - Frameless grill, suitable

for use with natural stone and

porcelain tiles.

**Manufacturer**

**Name: CCL Wetrooms**

**Contact Info: Address: Lodge Farm**

 **Hook Road**

 **North Warnborough**

 **Hook**

 **RG29 1HA**

 **Tel:** +44 (0)844 3276002 Fax: +44 (0)1256 765100

 **Web:** [www.ccl-wetrooms.co.uk](http://www.ccl-wetrooms.co.uk) Email: info@ccl-wetrooms.co.uk