Modular Wet-Floor

Product Specification Document

DATE: 16.07.2019 REF: PL-CW-PSDMWF01

A picture containing floor, indoor

Description automatically generated



A close up of a sign

Description automatically generatedA black sign with white text

Description automatically generated



# **Detailed Description**

The Modular Wet-Floor system can be used in a number of configurations to create a wetroom on a timber floor.

The system is versatile, cost effective and can be installed with the linear drain in either the centre of the shower area, or neatly positioned against the wall. Consisting of three main elements, the system is simple to configure.

# **System Components**

* Drainage component manufactured from tough ABS plastic
* 1200 mm wide tapered board (22–11mm) manufactured from XPS foam with a mineral coating
* Floor or wall grill (1.4401 [316] grade stainless steel) to suit wetroom layout

# **Features and Benefits**

* The drainage component and tapered boards can be easily trimmed on-site, making the whole system quick and easy to install. Two or more drainage components can be used to create larger shower areas.
* One or two way fall
* Create a shower area of any size
* Quick & easy to install
* Available with standard bottle trap or Lo-Seal waterless trap
* Centred, left or right handed trap position
* 360° rotatable outlet
* Flow rates of up to 68 L/min
* BBA Approved
* Height adjustable grill
* Grill lengths up to 2000mm
* Fast Track Bespoke service available – delivered in 3-4 days
* Lifetime guarantee

# **Product Guidance**

* The wall grill width is adjustable to allow for different wall tile thicknesses
* The height of the grill is adjustable in 1mm increments to suit tile thicknesses of between 6–20mm
* Additional spacers are available on request for tiles thicker than 20mm
* Floor grill width: 58mm
* Wall grill width: 86mm
* All grills are manufactured from 1.4401 (316) grade stainless steel and are available in a solid, slotted, stone-infill or frameless finish
* All grill finishes are available in 15 standard lengths from 600mm – 2000mm
* Bespoke grills can be manufactured for sizes that are in between or over the standard sizes
* Fast track bespoke lengths manufactured and delivered in 3-4 days

# **Options**

# **Waterproofing Membrane:**

CCL Wetrooms Tilesure Waterproofing & Decoupling Membrane should be applied to the entire wetroom floor, extending at least an additional metre outside of the shower area.

FWM (Flexible Wall Membrane) should then be applied to the walls within the shower area only, to a minimum height of 2000mm and overlapped onto the Tilesure/ Screedsure Reinforcing Tape.

See separate Product Specification Document for full details.

# **Product Specification**

**Product reference Code Traps Flow Rate**

TR50 Horizontal Trap MDC-1H 1 24 L/min

MDC-2H 2 41 L/min

MDC-3H 3 68 L/min

TR50 Vertical Trap MDC-1V 1 24 L/min

MDC-2V 2 41 L/min

MDC-3V 3 68 L/min

Waterless Trap MDC-W1 1 29 L/min

MDC-W2 2 56 L/min

MDC-W3 3 70 L/min

**Product reference Code Length Width**

Tapered Board MTB-03 300mm 1200mm

MTB-05 500mm 1200mm

MTB-07 700mm 1200mm

MTB-08 800mm 1200mm

MTB-09 900mm 1200mm

MTB-10 1000mm 1200mm

MTB-11 1100mm 1200mm

MTB-12 1200mm 1200mm

MTB-15 1500mm 1200mm

**Product reference Code Length Width**

Half Tapered Board MTB-H03 300mm 600mm

MTB-H05 500mm 600mm

MTB-H07 700mm 600mm

MTB-H08 800mm 600mm

MTB-H09 900mm 600mm

MTB-H10 1000mm 600mm

MTB-H11 1100mm 600mm

MTB-H12 1200mm 600mm

MTB-H15 1500mm 600mm

Tile Trim MTT-05 500mm

MTT-07 700mm

MTT-08 800mm

MTT-09 900mm

MTT-10 1000mm

MTT-11 1100mm

MTT-12 1200mm

MTT-15 1500mm

**Grill Type**

**Product reference Code Length Grill Finish**

Linear Wall Grill MWG-06 600mm Add code for Grill Finish

MWG-07 700mm

MWG-08 800mm

MWG-09 900mm

MWG-10 1000mm

MWG-11 1100mm

MWG-12 1200mm

MWG-13 1300mm

MWG-14 1400mm

MWG-15 1500mm

MWG-16 1600mm

MWG-17 1700mm

MWG-18 1800mm

MWG-19 1900mm

MWG-20 2000mm

MWG-FT Bespoke

MWG-BES Bespoke

Linear Floor Grill MFG-06 600mm Add code for Grill Finish

MFG-07 700mm

MFG-08 800mm

MFG-09 900mm

MFG-10 1000mm

MFG-11 1100mm

MFG-12 1200mm

MFG-13 1300mm

MFG-14 1400mm

**Product reference Code Length Grill Finish**

Linear Floor Grill MFG-15 1500mm Add code for Grill Finish

MFG-16 1600mm

MFG-17 1700mm

MFG-18 1800mm

MFG-19 1900mm

MFG-20 2000mm

MFG-FT Bespoke

MFG-BES Bespoke

Grill Finish Type A - Solid grill, grained

stainless steel with 5mm

gap around the grill.

Type B - Oblong slots, three

rows of oblong slots in a

grained stainless steel finish.

Type C - Square holes, three

rows of squares in a grained

stainless steel finish.

Type S8 – Stone-infill grill. Allows a

section of tile to be inserted to

provide a sleek continuous finish.

Suitable for 6-8mm stone/

porcelain tiles.

Type S12 – Stone-infill grill.

Suitable for 10-12mm stone/

porcelain tiles.

Type S20 – Stone-infill grill.

Suitable for 18-20mm stone/

porcelain tiles.

Type F - Frameless grill, suitable

for use with natural stone and

porcelain tiles.

**Manufacturer**

**Name: CCL Wetrooms**

**Contact Info: Address: Lodge Farm**

**Hook Road**

**North Warnborough**

**Hook**

**RG29 1HA**

**Tel:** +44 (0)844 3276002 Fax: +44 (0)1256 765100

**Web:** [www.ccl-wetrooms.co.uk](http://www.ccl-wetrooms.co.uk) Email: [info@ccl-wetrooms.co.uk](mailto:info@ccl-wetrooms.co.uk)