
FWM (Flexible Wall Membrane)

Product Specification Document

DATE: 25.07. 2019 REF: PL-CW-PSDFWM01









A black sign with white text

Description automatically generated

**Detailed Description**

FWM (Flexible Wall Membrane) has been developed for use onto walls, to provide waterproofing beneath ceramic, natural stone and porcelain tiles in bath/ shower rooms and other wet areas.

Pale blue, solvent free waterproof coating, suitable for use with Tilesure waterproofing and Decoupling Membrane or Screedsure waterproofing membrane. Junctions/ corners must be first reinforced with Reinforcing Tape as necessary.

**System Components**

FWM 8kg Tub

FWM Reinforcing Tape

FWM Primer

**Features and Benefits**

* Lifetime Guarantee
* Solvent free
* Quick and easy to apply
* Compatible with Tilesure and Screedsure
* Suitable for use on all commonly encountered substrates

**Preparation**

* All surfaces are to be clean, dry, free from dust, grease and oil, etc. Surfaces must be smooth, sound and flat, with all indentations filled with a suitable filler and all protrusions struck off
* Junctions/corners must be first reinforced with Reinforcing Tape as necessary

**Application**

* Single coat, brush or roller applied
* Coverage per coat (minimum 1 kg/m²)
* FWM-8: 8kg tub
* FWM should be applied to the walls of the shower area and overlapped onto the Tilesure Reinforcing Tape

# **Product specification**

**Product reference Code Size/Weight**

FWM FWM-08 8kg

FWM Reinforcing Tape FWM-TAPE 10m

FWM Primer FWM-PR5 500ml

**Manufacturer**

**Name: CCL Wetrooms**

**Contact Info: Address: Lodge Farm**

**Hook Road**

**North Warnborough**

**Hook**

**RG29 1HA**

**Tel:** +44 (0)844 3276002 Fax: +44 (0)1256 765100

**Web:** [www.ccl-wetrooms.co.uk](http://www.ccl-wetrooms.co.uk) Email: info@ccl-wetrooms.co.uk